The Amateur Radio Project - Inductance

# Inductance

### Question 2 of 10

The steady current through a 40mH inductor is doubled. The inductance will

1. decrease to 20mH
2. remain at 40mH
3. increase to 80mH
4. increase to 160mH

1 | 2 | 3 | 4

Back |

page (tq0502)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details