The Amateur Radio Project - Capacitance

# Capacitance

### Question 1 of 10

The parallel plates of a capacitor are separated by 2mm of air. If this separation is increased to 4 mm, the new value of capacitance will be

1. four times the original capacitance
2. double the original capacitance
3. one-half the original capacitance
4. one-quarter the original capacitance

1 | 2 | 3 | 4

Back |

page (tq0601)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details