# Transmission lines (feeders)

### Explanation of question 4

A feeder connected to an antenna measures resistance only at the transmitter end. The feeder is

1. matched
2. of too low impedance
3. of too high impedance
4. of incorrect length

The answer is :- 1 A pure resistance measurement indicates matching. A mismatch would be indicated by inductance or capacitance.

BACK

page (tq2004ex)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details