# Operating procedures and practices

### Explanation of question 18

For safety reasons a bleeder resistor is connected across a 0.5F capacitor. It should have a value

1. less than 500k
2. between 500k and 5M
3. between 5M and 10M
4. greater than 10M

The answer is :- 3 Paper dielectric capacitors are an example of low-leakage capacitors, i.e. they are able, in their isolated state, to store a charge for a considerable time. For this reason they should be individually short-circuited (time constant = RC).

BACK

page (tq2518ex)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details