The Amateur Radio Project - Diodes and their applications

# Diodes and their applications

### Question 8 of 14

A varactor diode is normally operated

1. forward-biased, and as a variable inductor
2. forward-biased, and as a variable capacitor
3. reverse-biased, and as a variable inductor
4. reverse-biased, and as a variable capacitor

1 | 2 | 3 | 4

Back |

page (tq1308)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd | Contact details