The Amateur Radio Project - Measurements

# Measurements

### Question 9 of 32

A moving coil instrument has an f.s.d. of 10mA and a resistance of 20. The value of multiplier resistance required to enable the instrument to read up to 12V will be

1. 1220
2. 1200
3. 1180
4. 18.8

   1. 1 | 2 | 3 | 4

      Back |

      page (tq2309)
      Some material Copyright John Bowyer G4KGS.
      Click here for important Copyright information
      Web Space provided by Hostroute.com Ltd | Contact details