This is a MS-DOS 7.10 boot disk for use with Coco and Dragon DOS based emulators. It is designed to give basic MS-DOS functionality for people who are running Windows XP/2000/NT with at least one FAT16 or FAT32 partition free for Coco/Dragon emulation use. To create the boot disk, insert a blank 1.44MB MS-DOS formatted disk in your floppy drive and double click on the correct file for your country. 

 
Boot Disk Features:

* Option to boot from floppy or hard drive.

* Start Menu.

* IDE CD-ROM support.

* Install to RAM disk to free up floppy drive.

* EMM386 memory management.

* Conventional, HMA, EMS, XMS and UMB memory available.

* 64K buffered direct memory access (DMA).

* FAT16 and FAT32 partition support.

* Long file name support.

* SmartDrive disk caching.

* Scandisk disk repair.

* MS-DOS tools.

* Serial/PS2 Mouse support.

* DOS "Reboot" command with support for flushing disk cache.

* PKWare's PKZIP 2.04g compression tools.

* Hex editors.

* Disk editor.

* PC turbo function emulator.

* Set emulator speed.

* Switch between standard and hi-res text modes.

* Hbreak for recovering from system crashes.

* Both US and UK versons supplied.


Minimum Requirements:

* IBM or compatible PC with 80386 microprocessor.

* 8MB RAM (4MB without RAM Disk).

* 1 x 2MB (DOS 1.44MB) floppy disk drive.

* Hard Drive (optional).


Some DOS based Coco/Dragon Emulators:

* David Keil's Coco Emulator.             
  http://discover-net.net/~dmkeil/

* Jeff Vavasour's Coco/Dragon Emulators.  
  http://www.vavasour.ca/jeff/trs80.html

* Paul Burgin's Coco/Dragon Emulators. 
  http://www.burgins.com/dragon.html

* Multi Emulator Super System.
  http://www.mess.org/




