    AST RESEARCH, INC.        TECHNICAL BULLETIN # 1651          01/07/97

    TITLE:  Ascentia P and Other Devices

    ISSUE

       After installing Windows 95, the user may find that the PCI
       bridge appears as an Other device in the Device Manager in
       Windows 95.

       This issue affects the following systems: 501996 and 501997.

    BACKGROUND

       This is an issue with the Intel Mobile Triton chipset.  The
       system is operating as designed. Windows 95 does not contain a
       specific driver for this PCI to PCI bridge. The standard driver
       will function in this case without any problems.

    ACTION

       1. Remove the question mark by selecting the PCI Bridge
          entry from

          /Control Panel/System/Device Manager/Other devices
          /PCI Bridge

       2. Select the Drivers tab and Change Drivers icon.

       3. Select System Devices and Standard PCI to PCI bridge.

       This will install drivers that allow the PCI bridge to appear
       under System Devices and will remove the Other device entry.

    NOTES

       N/A

    TAN EPR 1759AR

    ---------------------------------------------------------------------
    The information in this data sheet is subject to change without
    notice. AST Research, Inc. shall not be liable for technical or
    editorial errors or omissions contained herein; nor for incidental or
    consequential damages resulting from the furnishing, performance,
    or use of this material. This material contains information protected
    by copyright. No part of this material may be reproduced in any form
    without prior written consent from AST Research, Inc.
    All rights reserved.
    ---------------------------------------------------------------------
    Revision 01