    =

    AST RESEARCH, INC.          TECHNICAL BULLETIN # 1413               1-26-96

    =

    	   Ascentia 950N P75/P90/P120 and Installation of Windows 95

    PROBLEM

    During installation, Windows 95 does not properly detect the SVGA
    (800x600) LCD display panel properly.  When Windows 95 is installed on an
    Ascentia 950N P75/P90/P120 systems, the 11.8 TFT screen may come up in
    640x480 resolution.

    SOLUTION

    If the resolution is not correct after completing the Windows 95 installation,
    follow the steps below:

    1. Select "Settings" in the Display Properties window.
    2. In the desktop area, change the resolution from 640x480 to 800x600.
    3. Press "Change Display Type".
    4. Press "Monitor Type" and click on "Lap Top Display Panel (800x600).
    5. Press O.K.
    6. Press Close.
    7. Press Apply.

    SYSTEMS AFFECTED
    AST PART NUMBER AND DESCRIPTION

    501898-XXX      Ascentia 950N P/120 CTS 11.8

    Pentium is a Registered Trademark of Intel Corporation.