    =

    AST RESEARCH, INC.         TECHNICAL BULLETIN # 1357                11-9-95

    =

               Bravo MS OS/2 Unable to Install Mach64 Video Drivers

    PROBLEM

    OS/2 is unable to install ATI Mach 64 video drivers on the Bravo MS system.

    CAUSE

    ATI Mach64 video drivers that ship with OS/2 Warp are not compatible with
    systems that have 1 MB of video memory.

    SOLUTION

    Update the drivers by downloading the file MACH64.ZIP from IBM's BBS
    (919) 517-0001, "OS/2 Device Drivers" file area.  Follow the instructions in
    the README file.

    SYSTEMS AFFECTED
    AST PART NUMBER AND DESCRIPTION

    501815-XXX      Bravo MS P/133
    501814-XXX      Bravo MS P/120
    501774-XXX      Bravo MS P/100
    501534-XXX      Bravo MS P/90
    501772-XXX      Bravo MS P/75
    501701-XXX      Bravo MS P/75
    501651-XXX      Bravo MS-L P/90
    501702-XXX      Bravo MS-L P/75
    501860-XXX      Bravo MS-T P/133
    501778-XXX      Bravo MS-T P/120
    501777-XXX      Bravo MS-T P/100
    501660-XXX      Bravo MS-T P/90
    501703-XXX      Bravo MS-T P/75