    AST RESEARCH, INC.         TECHNICAL BULLETIN #0835               06-25-93

                 UPDATING THE VIDEO REFRESH RATE IN PREMMIA SYSTEMS

    PROBLEM:       The fields which allow updating of the video refresh rate do
                   not appear in the "View or Edit Details" screen in the EISA
                   Configuration Utility.

    CAUSE:         This is a design function of the EISA Configuration Utility
                   version 2.83 (part number 910743-032A).

    AFFECTED
    SYSTEMS:       All Premmia Systems.

    SOLUTION:      After starting the EISA Configuration Utility and choosing
                   "Configure Computer", choose "Step3.  Add or Remove Boards"
                   from the menu.  Add "AST Premmia Integrated VGA" as an
                   adapter.  Return to the "View or Edit Details" screen, where
                   the video refresh rate fields will appear under the "Embedded
                   AST Premmia VGA" field.