    =

    AST RESEARCH, INC.      TECHNICAL BULLETIN # 1285                   11-9-95

    =

                 Ascentia 950N and PCAnywhere 2.0 for Windows

    PROBLEM

    A PCAnywhere 2.0 session may disconnect when running an Ascentia 910N
    on battery.  The session will not, however, disconnect when running in turbo
    mode, or when connected to AC power.

    SOLUTION

    Update the PCAnywhere program to version 2.0C by downloading the file
    20UP_C.EXE from Symantec's forum on CompuServe (GO SYMANTEC).

    SYSTEMS AFFECTED
    AST PART NUMBER AND DESCRIPTION

    501707-XXX    Ascentia 950N P/75 CSS10
    501708-XXX    Ascentia 950N P/75 CTS10