    =

    AST RESEARCH, INC.         TECHNICAL BULLETIN # 1184               5-15-95

    =

    			  SLOW LOADING .NLM FILES UNDER NETWARE 3.11

    PROBLEM

    Under NetWare 3.11, the Manhattan P 5090 system may be excessively slow at
    loading .NLM modules from a DOS partition, after NCRSDMS3 is loaded.

    CAUSE

    The NCR driver does not support NetWare 3.11 in Manhattan systems.

    SYSTEMS AFFECTED
    AST PART NUMBER AND DESCRIPTION

    All Manhattan P and V systems.

    SOLUTION

    Edit the CONFIG.SYS file and add the statement

    DEVICE=

    Add NCR's DOSCAM.SYS to the CONFIG.SYS file.  DOSCAM.SYS improves the .NLM
    moudule's loading time from the DOS partition.  The DOSCAM.SYS file is on the
    NCR PCI SCSI Device Drivers diskette.

    This is ONLY a suggestion and ONLY under NetWare 3.11 with Manhattan
    P and V systems.