    AST RESEARCH, INC.         TECHNICAL BULLETIN #0680                  05-08-91

                         ETHERNEXT LAN CARD AND PREMIUM/286

    The Ethernext LAN card is not compatible with the Premium/286 when configured
    with a 3G Plus card and the system memory is set for zero wait states.

    When attempting to run application programs from the Novell 2.15 shell
    environment, a blank screen may appear.

    There is no resolution for this problem and Marketing has determined that
    this problem will not be resolved.