    =

    AST RESEARCH, INC.         TECHNICAL BULLETIN # 1291               11-28-95

    =

    		 Bravo MS P/75 and IBM Monochrome Printer Adapter

    PROBLEM

    The user is unable to set up the IBM monochrome printer adapter in the
    Bravo MS P/75 system BIOS.

    CAUSE

    The Bravo MS P/75 system does not support the IBM monochrome printer
    adapter card.

    SOLUTION

    Use a color printer adapter card that is able to emulate the monochrome mode.

    SYSTEMS AFFECTED
    AST PART NUMBER AND DESCRIPTION

    501749-XXX      BRAVO LC CX P100/3
    501772-XXX      BRAVO MS P/75
    501773-XXX      BRAVO MS P90/3
    501774-XXX      BRAVO MS P/100
    501775-XXX      BRAVO MS/L P75
    501776-XXX      BRAVO MS/L P100
    501777-XXX      BRAVO MS-T  P/100
    501778-XXX      BRAVO MS/T P120/3
    501784-XXX      BRAVO MS/T P75/3
    501814-XXX      BRAVO MS P/120
    501815-XXX      BRAVO MS P/133
    501816-XXX      BRAVO MS/L P120
    501841-XXX      BRAVO LC CX P120
    501860-XXX      BRAVO MS-T P/133
    501861-XXX      PIII+ P100 PRC
    501916-XXX      BRAVO MS P100/1000
    501926-XXX      PIII+ P133/1208