                                                             Last Revised
    AST RESEARCH, INC.        TECHNICAL BULLETIN # 1775          11/04/97

    TITLE:  Ascentia M, XGA LCD, Monitor Type

    ISSUE

       After performing a Hard Disk Restore on the XGA LCD, the
       resolution will be 800 x 600 instead of 1024 x 768.  .

       This issue affects the following Ascentia M systems: 503439,
       503433, and 503431.

    BACKGROUND

       N/A

    ACTION

       Change the monitor type and Desktop area as follows:

       1. Right-click the desktop and select Properties.

       2. Click Settings|Advanced|Monitor|Change.

       3. Select "Show All Devices".

       4. Select "Super VGA 1024x768" and click the [OK] button.

       5. Click [OK] button, then select desired Desktop area.

       6. Click [OK] button and follow the instructions on the
          screen.

    NOTES

       N/A

    TAN N/A

    ---------------------------------------------------------------------
    The information in this data sheet is subject to change without
    notice. AST Research, Inc. shall not be liable for technical or
    editorial errors or omissions contained herein; nor for incidental or
    consequential damages resulting from the furnishing, performance,
    or use of this material. This material contains information protected
    by copyright. No part of this material may be reproduced in any form
    without prior written consent from AST Research, Inc.
    All rights reserved.
    ---------------------------------------------------------------------
    Template Rev 02