    =

    AST RESEARCH, INC.          TECHNICAL BULLETIN # 1410               1-29-96

    =

    	  Ascentia 950N P90/P120 No Suspend in Windows For Workgroups

    PROBLEM

    The Ascentia 950N P90/P120 system may not suspend in Windows for
    Workgroups (WFW) if 32 bit access is enabled, and it is on a Logical Block
    Addressing (LBA) drive.

    SOLUTION

    Software suspend will not work automatically if the 32 bit access is disabled
    in virtual memory setup in WFW.  However, the system can be forced into
    Suspend mode manually by pressing the  and  keys.

    SYSTEMS AFFECTED
    AST PART NUMBER AND DESCRIPTION

    501897-XXX       Ascentia 950N P/120 CTS 10
    501898-XXX       Ascentia 950N P/120 CTS 11.8
    501741-XXX       Ascentia 950N P/90 CSS10
    501742-XXX       Ascentia 950N P/90 CT10
    501743-XXX       Ascentia 950N P/90 CTS10

    Pentium is a Registered Trademark of Intel Corporation.