    AST RESEARCH,                TECHNICAL BULLETIN #0896                 2-10-94

                      BRAVO NOTEBOOK MAINTENANCE MANUAL ERRORS

    Two errors exist in the Hardware Maintenance manual:

           1. In Appendix B it states that LPT1 is assigned to I/O address 03BCh.
              It should read address 0378H.

           2. In Appendix C it states that the video BIOS starts at address
              C000h.  It should read address E000h.

    This is an error in the manual only, the correct address will show up in your
    system setup.  Please note that the above corrections affect the following
    systems:

              SYSTEM                                  PART NUMBER

              Bravo NB 486SX/25                       501247-XXX
              Bravo NB 486SX/25 Color                 501248-XXX
              Bravo NB 486SX/25 ColorPlus             501249-XXX
              Advantage! Explorer 486SX/25 Mono       501262-XXX
              Advantage! Explorer 486SX/25 Color      501263-XXX
              Advantage! Explorer 486SX/25 ColorPlus  501264-XXX