    =

    AST RESEARCH, INC.          TECHNICAL BULLETIN # 1409                1-29-96

    =

    	     Ascentia 950N P90/P120 Kernel Trap Errors in Windows NT

    PROBLEM

    When running Windows NT 3.51, the Ascentia 950N P90/P120 system may fail,
    generating kernel trap errors while on battery power.

    SOLUTION

    To eliminate trap errors created while on battery power, run Windows NT in
    turbo mode   or on AC power.

    SYSTEMS AFFECTED
    AST PART NUMBER AND DESCRIPTION

    501897-XXX      Ascentia 950N P/120 CTS 10
    501898-XXX      Ascentia 950N P/120 CTS 11.8
    501741-XXX      Ascentia 950N P/90 CSS10
    501742-XXX      Ascentia 950N P/90 CT10
    501743-XXX      Ascentia 950N P/90 CTS10

    Pentium is a Registered Trademark of Intel Corporation.