    AST RESEARCH, INC.      TECHNICAL BULLETIN #1279        9/28/95

              ASCENTIA 950N DAMAGED SCREW HEAD ON MEMORY ACCESS DOOR

    PROBLEM:        The screw head to the memory access door is damaged.

    CAUSE:          The improper tool is being used to remove the screw.

    SOLUTION:       When removing the screw to the memory access door, use
    		a PH 0 or 1 screw driver.  Do not attempt to remove the
    		small screw using a large screw driver.  This will result
    		in damagaing the screw head, making it diffuclt to remove.