    =

    AST RESEARCH, INC.         TECHNICAL BULLETIN # 1376               12-19-95

    =

    	    Ascentia 950N Vibra16 Default Microphone Setting Too Low

    PROBLEM

    The recorded data may not be audible in the playback mode on the Ascentia
    950N system.

    CAUSE

    The default setting for the microphone volume level may be set too low (zero).

    SOLUTION

    Click on the Creative Mixer icon in the Audio group.  Move the slider bar up
    to the desired level.

    Please note that, increasing the volume to the maximum level may cause the
    speaker to feed back, during recording with the on-board microphone.

    SYSTEMS AFFECTED
    AST PART NUMBER AND DESCRIPTION

    501707-2XX      Ascentia 950N/75 CSS10 510/8
    501707-3XX      Ascentia 950N/75N CSS10 700/8
    501707-4XX      Ascentia 950N/75N CSS10 1G/8
    501708-3XX      Ascentia 950N/75N CT10 700/8
    501708-4XX      Ascentia 950N/975N CT10 1G/8