    AST RESEARCH, INC.         TECHNICAL BULLETIN #0769A                 11-10-92

                         AST SVGA 14" LOW RADIATION MONITOR

    PROBLEM:       When using the 1024x768 mode on the SVGA 14" low radiation
                   monitor, the picture will shift to the left.

    CAUSE:         This is due to a timing issue within the monitor itself.

    AFFECTED
    SYSTEMS:       SVGA 14" low radiation monitor part number  500902-XXX
                   revision A.

    SOLUTION:      Replace revision A monitor with a revision B monitor part
                   number 500902-001, 002, or 003.

    NOTE:  The part number 500902-XXX on the packing box will remain revision A.
           However, the part number on the monitor itself will change to 230253-
           XXX revision B.