    =

    AST RESEARCH, INC.         TECHNICAL BULLETIN # 1254                7-18-95

    =

    MANHATTAN P/V SFT III 4.1 INSTALLATION

    PROBLEM DESCRIPTION

    A user may experience difficulties when attempting to remirror an SFT III
    Manhattan P/V server during normal installation.  The completion of the
    remirroring process may be lengthy, depending on the size of the hard drives.

    Some SCSI controllers may exhibit the following problems during remirroring:

    remirroring stops
    or
    inoperable mirror group.

    SYSTEMS AFFECTED
    AST PART NUMBER AND DESCRIPTION

    501502-XXX MANHATTAN P 5090 - ALL MODELS
    501500-XXX MANHATTAN V 5090 - ALL MODELS

    SOLUTION

    This is only a recommendation.

    The followings are brief descriptions for the SFT III setup.

    Under normal installation:

    1. Setup a NetWare 4.1 server.
    2. Convert this NetWare 4.1 server to SFT III 4.1 server.
    3. During the conversion, the program will generate 3 installation disks for
       the second server.
    4. Copy these 3 disks to second server and follow through the questions.
    5. The second server will remirror with the first server.

    However, if any problems occur during the remirroring process, the user can
    activate the servers by doing the following:

    1. Run MSERVER on the first server.
    2. Load DSK, LAN and bind the ipx, and MSL drivers.

    At this point, the first server is waiting for a link.

    3. Run MSERVER on the second server.
    4. Load DSK, LAN and bind the ipx, and MSL drivers.

    At this point, the two servers are suppose to be synchronized.

    5. Type "activate server" from either server.
    6. Using  change to MSEngine and type "load install".
    7. Delete Mirrored drives.  Delete all NetWare partitions, and re-create the
       NetWare partitions.
    8. Create the Volume(s).
    9. Exit from installation menu and reload INSTALL.NLM from the DOS
       partition.
    10. Copy all the files ,license, and NDS.

    By doing so, the remirroring procedure will be avoided.