    AST RESEARCH, INC.        TECHNICAL BULLETIN # 1056                  1-24-95

    				  PREMMIA GX SCO UNIX INSTALLATION

    PROBLEM
    When attempting to install SCO UNIX (3.2 version 4.2) on the Premmia GX
    system, the system reports an unrecoverable disk error writing SCSI disk 0.

    CAUSE
    NCR SCSI Unix driver version 3.02 is not certified by SCO.

    SYSTEMS AFFECTED
    AST PART NUMBER       DESCRIPTION

    501457-601          PREMMIA GX P/90

    SOLUTION
    Use NCR SCSI SCO Unix driver version 3.03, P/N 911283-314.  Download file
    283314.EXE, from AST's BBS, "Systems" file area.  AST's BBS can be reached by
    dialing the following telephone numbers: (817) 230-6850.   AST's BBS supports
    modem speeds up to 28.8k bps.  The above files will also be posted on:

    	- CompuServe
    	  Go ASTSUPPORT

    	- AST Worldwide Web Site
    	  http://www.ast.com

    For additional information, see Software Bulletin 0171B on AST's BBS, in the
    SBS library.