    =

    AST RESEARCH, INC.         TECHNICAL BULLETIN # 1124                 4-4-95

    =

    				 PREMMIA MX 4-66D AND ARABIC WINDOWS

    PROBLEM

    ARABIC Windows 3.1 may not work with ATI MACH 64 release 1.03 video drivers
    on the Premmia MX 4-66D system.

    CAUSE

    File ATICNTL.DLL, release 1.03 of the ATI MACH 64 video drivers is
    incompatible with the Premmia MX system.

    SYSTEMS AFFECTED
    AST PART NUMBER AND DESCRIPTION

    501429-203     PREMMIA MX 4-66D

    SOLUTION

    Update the ATICNTL.DLL file with one dated 3/13/95 or later.  The version of
    the ATICNTL.DLL file will be included with the ATI MACH 64 video drivers,
    release 1.05.

    To install the driver, follow the steps below.

    1. Download ATICNTL.DLL from AST's BBS.

    2. Copy the file ATICNTL.DLL into your Windows directory.  This process will
    replace the current version that you are running.

    3. Start Windows, or if you are currently running Windows, exit and reboot the
    system.

    AST's BBS can be reached by dialing (817) 230-6850, in the "Systems" file
    area.  AST's BBS supports modem speeds up to 28.8k bps.  File ATICNTL.DLL
    will also be posted on:

    CompuServe
    Go ASTSUPPORT

    AST Worldwide Web Site
    http://www.ast.com