    =

    AST RESEARCH, INC.        TECHNICAL BULLETIN # 1195                 5-22-95

    =

    ASCENTIA 8XXN LOSS OF PCMCIA SUPPORT AFTER SUSPEND

    PROBLEM

    The Ascentia 8XXN system loses PCMCIA support after resuming from a zero-volt
    suspend.

    SYSTEMS AFFECTED
    AST PART NUMBER AND DESCRIPTION

    501469-XXX     ASCENTIA 800N 4/33
    501471-XXX     ASCENTIA 800N 4/50
    501683-XXX     ASCENTIA 810N 4/66 CS10

    SOLUTION

    Download file CS_APM.EXE from AST's BBS and add it to the system's
    AUTOEXEC.BAT file.  For information on editing AUTOEXEC.BAT, see the MS-DOS
    User's Guide shipped with the system.

    File CS_APM.EXE can be found on AST's BBS (817) 230-6850, in the "Systems"
    file area.  AST's BBS supports modem speeds up to 28.8k bps.
    The above file will also be posted on:

    CompuServe
    Go ASTSUPPORT

    AST Worldwide Web Site
    http://www.ast.com