    AST RESEARCH, INC.        TECHNICAL BULLETIN # 1664          02/11/97

    TITLE:  Ascentia 910N, ProStation, 3C509

    ISSUE

       If an Ascentia 910N is docked in a ProStation with a 3Com 3C509
       nic card installed, no servers are found when trying to logon to
       a network.

       This issue affects all Ascentia 910N systems.

    BACKGROUND

       N/A

    ACTION

       Configure the nic card to the following settings using 3Com's
       3C5X9CFG.EXE utility:

       I/O = 360

       IRQ = 9

       PNP = Disabled

    NOTES

       N/A

    TAN 001746CH, 000112BM

    ---------------------------------------------------------------------
    The information in this data sheet is subject to change without
    notice. AST Research, Inc. shall not be liable for technical or
    editorial errors or omissions contained herein; nor for incidental or
    consequential damages resulting from the furnishing, performance,
    or use of this material. This material contains information protected
    by copyright. No part of this material may be reproduced in any form
    without prior written consent from AST Research, Inc.
    All rights reserved.
    ---------------------------------------------------------------------
    Revision 01