    AST RESEARCH, INC.        TECHNICAL BULLETIN # 1054                  1-20-95

    			  ASCENTIA 900N AND INTEL LANSELECT SOFTWARE

    PROBLEM
    When running the LANSELECT software, if the temporary drive is located on the
    network, the Ascentia 900N system will hang after pressing .

    CAUSE
    There is an incompatibility between Intel's LANSELECT software and the
    Ascentia 900N system, when using a temporary drive on the network,

    SYSTEMS AFFECTED
    AST PART NUMBER    DESCRIPTION

    501299-2XX     ASCENTIA 900N 4/50 CS10
    501300-3XX     ASCENTIA 900N 4/50 CT9
    501302-2XX     ASCENTIA 900N 4/75 CS10
    501304-3XX     ASCENTIA 900N 4/75 CT10

    SOLUTION
    Set the LANSELECT temporary directory to the local hard drive.  For further
    information call Intel's Technical Support for LANSELECT at (503) 629-7000.