    =

    AST RESEARCH, INC.          TECHNICAL BULLETIN # 1211                6-7-95

    =

    ADVANTAGE! P60 OS/2 WARP AND LOGITECH MOUSE

    PROBLEM

    During installation of OS/2 Warp v3.0, the Logitech mouse (M-S28) is not
    detected.

    CAUSE

    The mouse driver that ships with OS/2 Warp v3.0 is not compatible with
    Logitech's mouse M-S28.

    SYSTEMS AFFECTED
    AST PART NUMBER AND DESCRIPTION

    501545-XXX          ADVANTAGE! P60

    SOLUTION

    Download file MOUSEWRP.EXE from AST's BBS (817) 230-6850, in the "Systems"
    file area.  AST's BBS supports modem speeds up to 28.8k bps.
    The above file will also be posted on:

    CompuServe
    Go ASTSUPPORT

    AST Worldwide Web Site
    http://www.ast.com

    After installation of OS/2 Warp v3.0, insert the diskette containing file
    MOUSEWRP.EXE into drive A.

    Open an OS/2 window.  Type

    A:

    and press .  Type

    Install

    This will replace the existing mouse driver with the Logitech mouse driver
    (part number 601036-0100 Rev. A).  Reboot the system.